The Institute for Technology Development Advanced Microelectronics Division 1 Research Boulevard, Suite 105 Starkville, Mississippi 39759 (601)325-2240 FAX (601)325-8144

SCMOS Standard Cell Library

1 April 1989

Version 2.0

Cell Old Cell Name Name Description

norf401 1140 4 Input NOR oaif2201 1860 2, 2 OR/NAND Mux orf401 1740 4 Input OR pudf000 1440 Pull-Down puuf000 1430 Pull-Up swcf020 1370 Transmission Gate via 8680 Wiring Via xnof201 2350 Exclusive NOR �xnsf201 Static Exclusive NOR xorf201 2310 Exclusive OR �xosf201 Static Exclusive NOR

� This cell uses a static CMOS implementation that can be simulated by IRSIM.

The Institute for Technology Development Advanced Microelectronics Division 1 Research Boulevard, Suite 105 Starkville, Mississippi 39759 (601)325-2240 FAX (601)325-8144

SCMOS Standard Cell Library

1 April 1989

Version 2.0

Library Description

Cell Old Cell Name Name Description

aof2201 1970 2, 2 AND/OR Mux aof2301 1930 2, 3 AND/OR Mux aof3201 1810 3, 2 AND/OR Mux aof4201 1910 4, 2 AND/OR Mux aoif2201 1870 2, 2 AND/NOR Mux blf00001 1880 2, 1 AND/NOR Mux blf00101 1890 2, 1 OR/NAND Mux buff100 1550 High Impedance Buffer buff101 1320 Non-Inverting Buffer buff121 1340 Tri-State Buffer delf011 1560 Delay Cell dfbf311 1480 D-Flip Flop with S, R, Q & QB dfnf311 1830 D-Flip Flop with Q & QB dfrf301 1570 D-Flip Flop with Asynchronous R & Q dfrf311 1580 D-Flip Flop with Asynchronous R, Q & QB faf001 1850 Full Adder feed 8630 Buss Crosser invf100 1540 High Impedance Inverter invf101 1310 Inverter invf103 1330 3X Inverting Buffer invf104 1520 4X Inverting Buffer invf201 1100 Dual Inverter labf111 1410 NAND Latch labf211 1420 NOR Latch larf310 1530 Clocked Latch ldf001 8660 RC Load Cell muxf201 1350 Data Select nanf201 1220 2 Input NAND nanf211 1660 2 Input NAND/AND nanf251 1620 A OR B-not Decoder nanf301 1230 3 Input NAND nanf311 1670 3 Input NAND/AND nanf401 1240 4 Input NAND nanf411 1680 4 Input NAND/AND norf201 1120 2 Input NOR norf211 1760 2 Input OR/NOR norf251 1610 A-not AND B Decoder norf301 1130 3 Input NOR norf311 1770 3 Input OR/NOR