\begin{verbatim}
	Placement Of MacroCells using Simulated Annealing
	VERSION 4.4 With ACS : Tue Feb 28 14:34:40 PST 1989
	SEQUENTIAL VERSION
puppy [options] cell-name:view-name
  -o cell:view    Specify output cell and view
  -O number       Overlap     Weight in SA cost function [1.00]
  -W number       Wire Length Weight in SA cost function [1.00]
  -A number       Area        Weight in SA cost function [1000.00]
  -C number       ConstrViolations Weight in SA cost function [1.00]
  -T number       Starting Temperature for SA [automatic]
  -R number       Seed for the random number generator
  -S number       Cooling Schedule (0,1,2)
  -a number       Moves per annealing variable [20]
  -x number       Set expansion factor for the cells [2.00]
  -c              Compute the cost of current placement and stop
  -f              Place only floating terminals
  -q              Disable the translations
  -t              Disable the transformations
  -g              Turn OFF graphic output
  -l [CNB]        List C_ells or N_ets or B_oth. Also writes parPuppy file
  -d              Enables debug
(Command line options override the values in the parPuppy file)
\end{verbatim}
